{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MV"]
[]
[]
[]
[]
["","","","","","AZAS100MUV","AZAS140MUV"]
["Dimensions","Unit","","Height","mm","990","990"]
["","","","Width","mm","940","940"]
["","","","Depth","mm","320","320"]
["Weight","Unit","","","kg","72","79"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","15.5","15.5"]
["Sound power level","Cooling","","","dBA","70","73"]
["","Heating","","","dBA","","73 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","53","54"]
["","Heating","","Nom.","dBA","57","57"]
["Refrigerant","Type","","","","R-32","R-32"]
["","Charge","","","kg","2.6","2.9"]
["","GWP","","","","675","675"]
["","Charge","","","tCO2Eq","1.76","1.96"]
["Piping connections","Liquid","","OD","mm","9.52","9.52"]
["","Gas","","OD","mm","15.9","15.9"]
["","Piping length","OU - IU","Max.","m","30","30"]
["","","System","Equivalent","m","50","50"]
["","","","Chargeless","m","30","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","m","30","30"]
["","","IU - IU","Max.","m","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","LOT10 Energy Label","","","","1","1"]
["","Declaration of conformity","","","","2","2"]
["","Tie-wraps","","","","2","2"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","25","32"]
["Notes","","","","","(1) - According to ENER Lot 21","(1) - According to ENER Lot 21"]
["","","","","","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]
["","","","","","(3) - Ssc: Short-circuit power","(3) - Ssc: Short-circuit power"]
["","","","","","(4) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current ≤ 16A per phase.","(4) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current ≤ 16A per phase."]