{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A8"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B8"]
["Cooling capacity","Nom.","","kW","5"]
["Heating capacity","Nom.","","kW","5.8"]
["Nominal efficiency","EER","","","3"]
["","COP","","","2.99"]
["","Annual energy consumption","","kWh","833"]
["","Energy labeling Directive","Cooling","","C"]
["","","Heating","","D"]
["Space cooling","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","5"]
["","SEER","","","5.7"]
["","Annual energy consumption","","kWh/a","307"]
["Space heating (Average climate)","Energy efficiency class","","","A"]
["","Capacity","Pdesign","kW","4"]
["","SCOP/A","","","3.89"]
["","Pdh Heating capacity at -10°","","kW","3.11"]
["","Annual energy consumption","","kWh/a","1440"]
["Notes","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data"]