{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":61,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA100AVEB / RZQG71L8Y1B","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZQG71L8Y1B","FHA35AVEB9 / FHA35AVEB9 / RZQG71L8Y1B","FHA71AVEB9 / RZQG71L8Y1B","FHA50AVEB9 / FHA50AVEB9 / RZQG71L8Y1B","FHA50AVEB98 / FHA50AVEB98 / RZQG71L8Y1B","FHA71AVEB98 / RZQG71L8Y1B","FHA100AVEB8 / RZQG71L8Y1B","FHA35AVEB98 / FHA35AVEB98 / RZQG71L8Y1B","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZQG71L8Y1B","FHA140AVEB / RZQG140L7Y1B","FHA140AVEB8 / RZQG140L7Y1B","FHA100AVEB / RZQG100L8Y1B (Archived)","FHA100AVEB8 / RZQG100L8Y1B (Archived)","FHA100AVEB9 / RZQG100L8Y1B (Archived)","FHA125AVEB / RZQG125L8Y1B (Archived)","FHA125AVEB8 / RZQG125L8Y1B (Archived)","FHA125AVEB9 / RZQG125L8Y1B (Archived)","FHA140AVEB / RZQG100L8Y1B (Archived)","FHA140AVEB / RZQG125L8Y1B (Archived)","FHA140AVEB8 / RZQG100L8Y1B (Archived)","FHA140AVEB8 / RZQG125L8Y1B (Archived)","FHA140AVEB9 / RZQG100L8Y1B (Archived)","FHA140AVEB9 / RZQG125L8Y1B (Archived)","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZQG100L8Y1B (Archived)","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZQG125L8Y1B (Archived)","FHA50AVEB9 / FHA50AVEB9 / FHA50AVEB9 / RZQG125L8Y1B (Archived)","FHA50AVEB9 / FHA50AVEB9 / RZQG100L8Y1B (Archived)","FHA60AVEB9 / FHA60AVEB9 / RZQG125L8Y1B (Archived)","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZQG100L8Y1B (Archived)","FHA50AVEB9 / FHA50AVEB9 / FHA50AVEB9 / RZQG100L8Y1B (Archived)","FHA71AVEB9 / FHA71AVEB9 / RZQG100L8Y1B (Archived)","FHA71AVEB9 / FHA71AVEB9 / RZQG125L8Y1B (Archived)","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZQG125L8Y1B (Archived)","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZQG100L8Y1B (Archived)","FHA50AVEB99 / FHA50AVEB99 / FHA50AVEB99 / RZQG125L8Y1B (Archived)","FHA50AVEB99 / FHA50AVEB99 / RZQG100L8Y1B (Archived)","FHA60AVEB99 / FHA60AVEB99 / RZQG125L8Y1B (Archived)","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZQG100L8Y1B (Archived)","FHA50AVEB99 / FHA50AVEB99 / FHA50AVEB99 / RZQG100L8Y1B (Archived)","FHA71AVEB99 / FHA71AVEB99 / RZQG100L8Y1B (Archived)","FHA71AVEB99 / FHA71AVEB99 / RZQG125L8Y1B (Archived)","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZQG125L8Y1B (Archived)","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZQG100L8Y1B (Archived)","FHA50AVEB98 / FHA50AVEB98 / FHA50AVEB98 / RZQG125L8Y1B (Archived)","FHA50AVEB98 / FHA50AVEB98 / RZQG100L8Y1B (Archived)","FHA60AVEB98 / FHA60AVEB98 / RZQG125L8Y1B (Archived)","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZQG100L8Y1B (Archived)","FHA50AVEB98 / FHA50AVEB98 / FHA50AVEB98 / RZQG100L8Y1B (Archived)","FHA71AVEB98 / FHA71AVEB98 / RZQG100L8Y1B (Archived)","FHA71AVEB98 / FHA71AVEB98 / RZQG125L8Y1B (Archived)","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZQG71L8Y1B (Archived)","FHA35AVEB99 / FHA35AVEB99 / RZQG71L8Y1B (Archived)","FHA71AVEB99 / RZQG71L8Y1B (Archived)","FHA100AVEB9 / RZQG71L8Y1B (Archived)","FHA50AVEB99 / FHA50AVEB99 / RZQG71L8Y1B (Archived)","FHA140AVEB9 / RZQG140L7Y1B (Archived)"]
["Cooling capacity","Nom.","","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","13.40","13.40","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Space cooling","SEER","","","6.86","5.10","5.10","6.86","5.10","5.10","6.86","6.86","5.10","5.10","6.22","6.22","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","5.10","5.10","6.86","6.86","5.10","6.22"]
["","Annual energy consumption","","kWh/a","347","467","467","347","467","467","347","347","467","467","1,292","1,292","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","467","467","347","347","467","1,292"]
["","Capacity","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","13.40","13.40","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","Energy efficiency class","","","A++","A","A","A++","A","A","A++","A++","A","A","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A","A","A++","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","6.00","6.00","7.60","6.00","6.00","7.60","7.60","6.00","6.00","11.61","11.61","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","6.00","6.00","7.60","7.60","6.00","11.61"]
["","SCOP/A","","","4.32","3.80","3.80","4.32","3.80","3.80","4.32","4.32","3.80","3.80","4.22","4.22","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","3.80","3.80","4.32","4.32","3.80","4.22"]
["","Energy efficiency class","","","A+","A","A","A+","A","A","A+","A+","A","A","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A","A","A+","A+","A"]
["","Annual energy consumption","","kWh/a","2,463","2,211","2,211","2,463","2,211","2,211","2,463","2,463","2,211","2,211","3,851","3,851","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","2,211","2,211","2,463","2,463","2,211","3,851"]
["Nominal efficiency","EER","","","3.82","3.30","3.30","3.82","3.30","3.30","3.82","3.82","3.30","3.30","2.92","2.92","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","3.30","3.30","3.82","3.82","3.30","2.92"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range"]
["","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data"]
["Nominal efficiency","Annual energy consumption","","kWh","","","","890","","","890","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","890"]
["","COP","","","","","","4.13","","","4.13","","","","3.63","3.63","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","4.13","","","3.63"]
["","Energy labeling Directive","Cooling","","","","","A","","","A","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A"]
["","","Heating","","","","","A","","","A","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A"]
["Heating capacity","Nom.","","kW","","","","7.50","","","7.50","","","","15.50","15.50","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","7.50","","","15.50"]
["Space cooling","ηs,c","","%","","","","","","","","","","","245.96"]
["Space heating (Average climate)","ηs,h","","%","","","","","","","","","","","165.87"]
["Energy Efficiency Range","","","","","","","","","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]