{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":20,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A / RXF-A"]
[]
[]
[]
[]
["","","","","FTXF20A2V1B / RXF20A2V1B","FTXF20A2V1B / RXF20A5V1B","FTXF20A5V1B / RXF20A2V1B","FTXF20A5V1B / RXF20A5V1B","FTXF25A2V1B / RXF25A2V1B","FTXF25A2V1B / RXF25A5V1B","FTXF25A5V1B / RXF25A2V1B","FTXF25A5V1B / RXF25A5V1B","FTXF35A2V1B / RXF35A2V1B","FTXF35A2V1B / RXF35A5V1B","FTXF35A5V1B / RXF35A2V1B","FTXF35A5V1B / RXF35A5V1B","FTXF50A2V1B / RXF50A2V1B","FTXF60A2V1B / RXF60A2V1B","FTXF71A2V1B / RXF71A2V1B","FTXF71A2V1B / RXF71A5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.7","1.7","2.30","2.30"]
["","Max.","","kW","2.6","2.6","2.6","2.6","3.0","3.0","3.0","3.0","3.8","3.8","3.8","3.8","6.0","7.0","7.30","7.30"]
["","Nom.","","kW","2.00","2.00","2.00","2.00","2.50","2.50","2.50","2.50","3.30","3.30","3.30","3.30","5.00","6.00","7.10","7.10"]
["Space cooling","SEER","","","6.15","6.15","6.15","6.15","6.22","6.22","6.22","6.22","6.21","6.21","6.21","6.21","6.21","6.15","5.15","5.15"]
["","Annual energy consumption","","kWh/a","114","114","114","114","141","141","141","141","197","197","197","197","282","342","483","483"]
["","Capacity","Pdesign","kW","2.00","2.00","2.00","2.00","2.50","2.50","2.50","2.50","3.50","3.50","3.50","3.50","5.00","6.00","7.10","7.10"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.20","2.20","2.20","2.40","2.40","2.40","2.40","2.80","2.80","2.80","2.80","4.60","4.80","6.20","6.20"]
["","SCOP/A","","","4.10","4.10","4.10","4.10","4.06","4.06","4.06","4.06","4.06","4.06","4.06","4.06","4.06","4.06","3.81","3.81"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A","A"]
["","Pdh Heating capacity at -10°","","kW","1.99","1.99","1.99","1.99","2.10","2.10","2.10","2.10","2.33","2.33","2.33","2.33","4.12","4.24","5.02","5.02"]
["","Annual energy consumption","","kWh/a","751","751","751","751","827","827","827","827","965","965","965","965","1,584","1,655","2,278","2,278"]
["Nominal efficiency","Annual energy consumption","","kWh","","","","","","","","","","","","","","","1,387","1,387"]
["","EER","","","3.94","3.94","3.94","3.94","3.30","3.30","3.30","3.30","3.30","3.30","3.30","3.30","3.33","3.25","2.56","2.56"]
["","COP","","","4.19","4.19","4.19","4.19","4.01","4.01","4.01","4.01","3.71","3.71","3.71","3.71","3.71","3.93","3.15","3.15"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","E","E"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","D","D"]
["Heating capacity","Nom.","","kW","2.50","2.50","2.50","2.50","2.80","2.80","2.80","2.80","3.50","3.50","3.50","3.50","6.00","6.40","8.20","8.20"]
["","Min.","","kW","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.30","1.70","1.70","2.30","2.30"]
["","Max.","","kW","3.50","3.50","3.50","3.50","4.00","4.00","4.00","4.00","4.80","4.80","4.80","4.80","7.70","8.00","9.00","9.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","","","","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]