{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ20A2V1BB / RXJ20M5V1B9 (Archived)","FTXJ25A2V1BB / RXJ25M5V1B9 (Archived)","FTXJ35A2V1BB / RXJ35M5V1B9 (Archived)"]
["Cooling capacity","Nom.","","kW","3.50"]
["Space cooling","SEER","","","7.19"]
["","Annual energy consumption","","kWh/a","170"]
["","Capacity","Pdesign","kW","3.50"]
["","Energy efficiency class","","","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.00"]
["","SCOP/A","","","4.60"]
["","Energy efficiency class","","","A++"]
["","Pdh Heating capacity at -10°","","kW","2.61"]
["","Annual energy consumption","","kWh/a","913"]
["Nominal efficiency","Annual energy consumption","","kWh","428"]
["","EER","","","4.09"]
["","COP","","","4.04"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Heating capacity","Nom.","","kW","4.00"]
["Notes","","","","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","","RXJ20M5V1B9","RXJ25M5V1B9","RXJ35M5V1B9"]
["Cooling capacity","Nom.","","kW","","2.30","2.40","3.50"]
["Heating capacity","Nom.","","kW","","2.50","3.20","4.00"]
["Nominal efficiency","EER","","","","4.64","4.73","4.09"]
["","COP","","","","5.00","4.57","4.04"]
["","Annual energy consumption","","kWh","","248","254","428"]
["","Energy labeling Directive","Cooling","","","A","A","A"]
["","","Heating","","","A","A","A"]
["Space cooling","Energy efficiency class","","","","A+++","A+++","A++"]
["","Capacity","Pdesign","kW","","2.30","2.40","3.50"]
["","SEER","","","","8.73","8.64","7.19"]
["","Annual energy consumption","","kWh/a","","92","97","170"]
["Space heating (Average climate)","Energy efficiency class","","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","","2.10","2.70","3.00"]
["","SCOP/A","","","","4.61","4.60","4.60"]
["","Pdh Heating capacity at -10°","","kW","","1.80","2.18","2.61"]
["","Annual energy consumption","","kWh/a","","638","822","913"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]