{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BS / RXJ20M5V1B9 (Archived)","FTXJ25A2V1BS / RXJ25M5V1B9 (Archived)","FTXJ35A2V1BS / RXJ35M5V1B9 (Archived)"]
["Outdoor unit","","","","RXJ20M5V1B9","RXJ25M5V1B9","RXJ35M5V1B9"]
["Cooling capacity","Nom.","","kW","2.30","2.40","3.50"]
["Heating capacity","Nom.","","kW","2.50","3.20","4.00"]
["Nominal efficiency","EER","","","4.64","4.73","4.09"]
["","COP","","","5.00","4.57","4.04"]
["","Annual energy consumption","","kWh","248","254","428"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++","A++"]
["","Capacity","Pdesign","kW","2.30","2.40","3.50"]
["","SEER","","","8.73","8.64","7.19"]
["","Annual energy consumption","","kWh/a","92","97","170"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","2.10","2.70","3.00"]
["","SCOP/A","","","4.61","4.60","4.60"]
["","Pdh Heating capacity at -10°","","kW","1.80","2.18","2.61"]
["","Annual energy consumption","","kWh/a","638","822","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]