{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AW / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BW / RXJ20M5V1B9","FTXJ25A2V1BW / RXJ25M5V1B9"]
["Cooling capacity","Nom.","","kW","2.30","2.40"]
["Space cooling","SEER","","","8.73","8.64"]
["","Annual energy consumption","","kWh/a","92","97"]
["","Capacity","Pdesign","kW","2.30","2.40"]
["","Energy efficiency class","","","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.10","2.70"]
["","SCOP/A","","","4.61","4.60"]
["","Energy efficiency class","","","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","1.80","2.18"]
["","Annual energy consumption","","kWh/a","638","822"]
["Nominal efficiency","Annual energy consumption","","kWh","248","254"]
["","EER","","","4.64","4.73"]
["","COP","","","5.00","4.57"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","2.50","3.20"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]