{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 2MXM-A8"]
[]
[]
[]
[]
["","","","","FTXM25N2V1B / FTXM25N2V1B / 2MXM50A2V1B8","FTXM20N2V1B / FTXM50N2V1B / 2MXM68A2V1B8","FTXM25N2V1B / FTXM42N2V1B / 2MXM68A2V1B8","FTXM35N2V1B / FTXM35N2V1B / 2MXM68A2V1B8"]
["Cooling capacity","Nom.","","kW","5.00","6.8","6.7","6.8"]
["Heating capacity","Nom.","","kW","5.60","8.60","8.30","8.60"]
["Nominal efficiency","EER","","","4.01","3.59","3.74","3.94"]
["","COP","","","4.08","3.82","3.95","3.81"]
["","Annual energy consumption","","kWh","623","947","896","863"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A+++","A++","A++","A++"]
["","Capacity","Pdesign","kW","5.00","6.80","6.70","6.80"]
["","SEER","","","8.53","6.75","6.94","6.97"]
["","Annual energy consumption","","kWh/a","205","353","338","342"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A","A","A+"]
["","Capacity","Pdesign","kW","4.20","4.50","4.30","4.80"]
["","SCOP/A","","","4.61","3.90","3.86","4.00"]
["","Pdh Heating capacity at -10°","","kW","3.20","3.55","3.41","3.73"]
["","Annual energy consumption","","kWh/a","1,275","1614","1560","1680"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]