{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":14,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 4MXM-N"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / 4MXM68N2V1B","FTXM20N2V1B / FTXM50N2V1B / 4MXM68N2V1B","FTXM35N2V1B / FTXM35N2V1B / 4MXM68N2V1B","FTXM20N2V1B / FTXM20N2V1B / FTXM42N2V1B / 4MXM80N2V1B","FTXM20N2V1B / FTXM25N2V1B / FTXM35N2V1B / 4MXM80N2V1B","FTXM20N2V1B / FTXM60N2V1B / 4MXM80N2V1B","FTXM35N2V1B / FTXM42N2V1B / 4MXM80N2V1B","FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 4MXM68N2V1B (Archived)","FTXM25N2V1B / FTXM42N2V1B / 4MXM68N2V1B (Archived)","FTXM20N2V1B / FTXM20N2V1B / FTXM20N2V1B / FTXM20N2V1B / 4MXM80N2V1B (Archived)"]
["Cooling capacity","Nom.","","kW","6.5","6.8","6.8","8.20","7.40","7.40","7.70"]
["Space cooling","SEER","","","7.76","7.78","8.02","8.07","8.19","7.38","7.40"]
["","Annual energy consumption","","kWh/a","294","306","297","356","317","351","365"]
["","Capacity","Pdesign","kW","6.50","6.80","6.80","8.20","7.40","7.40","7.70"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","5.30","4.50","4.80","5.37","5.37","4.27","4.27"]
["","SCOP/A","","","4.09","3.90","4.00","3.93","3.95","4.05","4.05"]
["","Energy efficiency class","","","A+","A","A+","A","A","A+","A+"]
["","Annual energy consumption","","kWh/a","1,814","1,612","1,680","1,913","1,902","1,474","1,475"]
["Nominal efficiency","EER","","","4.01","4.28","4.70","4.58","4.94","4.61","4.58"]
["","Annual energy consumption","","kWh","810","794","723","895","749","803","841"]
["","COP","","","4.49","3.82","3.81","3.91","3.90","3.85","3.35"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","C"]
["Heating capacity","Nom.","","kW","8.20","8.60","8.60","9.40","9.30","9.30","9.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","","","","6.8","6.7","7.40"]
["Heating capacity","Nom.","","kW","","","","","","","","8.60","8.30","9.60"]
["Nominal efficiency","EER","","","","","","","","","","3.85","4.46","4.57"]
["","COP","","","","","","","","","","4.38","3.95","4.97"]
["","Annual energy consumption","","kWh","","","","","","","","883","751","810"]
["","Energy labeling Directive","Cooling","","","","","","","","","A","A","A"]
["","","Heating","","","","","","","","","A","A","A"]
["Space cooling","Energy efficiency class","","","","","","","","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","","","6.80","6.70","7.40"]
["","SEER","","","","","","","","","","7.71","7.99","8.32"]
["","Annual energy consumption","","kWh/a","","","","","","","","309","294","311"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","A+","A","A+"]
["","Capacity","Pdesign","kW","","","","","","","","5.30","4.30","6.23"]
["","SCOP/A","","","","","","","","","","4.10","3.86","4.55"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","","4.22","3.41","4.86"]
["","Annual energy consumption","","kWh/a","","","","","","","","1807","1559","1915"]