{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":46,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / FTXM35R2V1B / 2MXM40A2V1B9","FTXM20R2V1B / FTXM25R2V1B / 2MXM40A2V1B9","FTXM20R2V1B / FTXM35R2V1B / 2MXM40A2V1B9","FTXM25R2V1B / FTXM25R2V1B / 2MXM40A2V1B9","FTXM20R5V1B / FTXM35R5V1B / 2MXM40A2V1B9","FTXM20R5V1B / FTXM25R5V1B / 2MXM40A2V1B9","FTXM25R5V1B / FTXM35R5V1B / 2MXM40A2V1B9","FTXM25R5V1B / FTXM25R5V1B / 2MXM40A2V1B9","FTXM20R2V1B / FTXM20R2V1B / 2MXM40A2V1B9","FTXM20R5V1B / FTXM20R5V1B / 2MXM40A2V1B9","FTXM35R2V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM35R2V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM35R2V1B / FTXM35R2V1B / 2MXM50A2V1B9","FTXM35R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM20R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM25R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM35R2V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM42R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM35R5V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM35R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM42R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM20R5V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM25R5V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM25R2V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM25R5V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM50R2V1B / 2MXM68A2V1B9","FTXM20R5V1B / FTXM50R2V1B / 2MXM68A2V1B9","FTXM25R2V1B / FTXM42R2V1B / 2MXM68A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 2MXM68A2V1B9","FTXM35R2V1B / FTXM35R2V1B / 2MXM68A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 2MXM68A2V1B9"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","","","5.00","5.00","5.00","5.00","5.00","4.00","5.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","4.00","4.50","5.00"]
["Space cooling","SEER","","","8.11","8.50","8.19","8.36","8.19","8.50","8.11","8.36","","","8.53","8.54","8.58","8.58","8.60","8.71","8.54","8.68","8.51","8.56","8.52","8.57","8.54","8.51","8.56","8.52","8.58","8.53","8.58","8.60","8.57","8.71","8.68","8.54"]
["","Annual energy consumption","","kWh/a","173","165","171","168","171","165","173","168","","","205","205","204","204","203","161","205","181","206","204","205","204","205","206","204","205","204","205","204","203","204","161","181","205"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","","","5.00","5.00","5.00","5.00","5.00","4.00","5.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","4.00","4.50","5.00"]
["","Energy efficiency class","","","A++","A+++","A++","A++","A++","A+++","A++","A++","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","3.20","3.20","3.20","3.20","","","4.20","4.20","4.20","4.20","4.20","4.00","4.20","4.10","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.00","4.10","4.20"]
["","SCOP/A","","","4.61","4.60","4.60","4.60","4.60","4.60","4.61","4.60","","","4.73","4.61","4.65","4.63","4.64","4.61","4.61","4.61","4.66","4.62","4.69","4.67","4.61","4.66","4.62","4.69","4.65","4.73","4.63","4.64","4.67","4.61","4.61","4.61"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.59","2.56","2.58","2.57","2.58","2.56","2.59","2.57","","","3.25","2.86","2.91","2.93","2.95","2.81","2.88","2.83","3.17","2.89","3.21","2.97","2.88","3.17","2.89","3.21","2.91","3.25","2.93","2.95","2.97","2.81","2.83","2.86"]
["","Annual energy consumption","","kWh/a","971","973","974","974","974","973","971","974","","","1,243","1,275","1,265","1,269","1,266","1,216","1,277","1,246","1,261","1,272","1,255","1,259","1,277","1,261","1,272","1,255","1,265","1,243","1,269","1,266","1,259","1,216","1,246","1,275"]
["Nominal efficiency","Annual energy consumption","","kWh","472","481","476","478","476","481","472","478","","","598","619","611","608","604","471","614","534","608","616","605","601","614","608","616","605","611","598","608","604","601","471","534","619"]
["","EER","","","4.24","4.16","4.20","4.18","4.20","4.16","4.24","4.18","","","4.18","4.04","4.09","4.11","4.14","4.25","4.07","4.21","4.11","4.06","4.13","4.16","4.07","4.11","4.06","4.13","4.09","4.18","4.11","4.14","4.16","4.25","4.21","4.04"]
["","COP","","","4.46","4.32","4.41","4.37","4.41","4.32","4.46","4.37","","","3.94","4.12","4.03","4.01","4.00","4.09","4.13","4.10","4.15","4.05","3.98","3.98","4.13","4.15","4.05","3.98","4.03","3.94","4.01","4.00","3.98","4.09","4.10","4.12"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","","","5.60","5.60","5.60","5.60","5.60","5.20","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.20","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","","","","","4","4","","","","","","","","","","","","","","","","","","","","","","","","","5","5","6.8","6.8","6.7","6.7","6.8","6.8"]
["Heating capacity","Nom.","","kW","","","","","","","","","4.2","4.2","","","","","","","","","","","","","","","","","","","","","","","","","5.6","5.6","8.60","8.60","8.30","8.30","8.60","8.60"]
["Nominal efficiency","EER","","","","","","","","","","","4.3","4.3","","","","","","","","","","","","","","","","","","","","","","","","","4.01","4.01","3.59","3.59","3.74","3.74","3.94","3.94"]
["","COP","","","","","","","","","","","4.28","4.28","","","","","","","","","","","","","","","","","","","","","","","","","4.08","4.08","3.82","3.82","3.95","3.95","3.81","3.81"]
["","Annual energy consumption","","kWh","","","","","","","","","465","465","","","","","","","","","","","","","","","","","","","","","","","","","623","623","947","947","896","896","863","863"]
["","Energy labeling Directive","Cooling","","","","","","","","","","A","A","","","","","","","","","","","","","","","","","","","","","","","","","A","A"]
["","","Heating","","","","","","","","","","A","A","","","","","","","","","","","","","","","","","","","","","","","","","A","A"]
["Space cooling","Energy efficiency class","","","","","","","","","","","A+++","A+++","","","","","","","","","","","","","","","","","","","","","","","","","A+++","A+++","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","","","","4","4","","","","","","","","","","","","","","","","","","","","","","","","","5","5","6.80","6.80","6.70","6.70","6.80","6.80"]
["","SEER","","","","","","","","","","","8.53","8.53","","","","","","","","","","","","","","","","","","","","","","","","","8.53","8.53","6.75","6.75","6.94","6.94","6.97","6.97"]
["","Annual energy consumption","","kWh/a","","","","","","","","","164","164","","","","","","","","","","","","","","","","","","","","","","","","","205","205","353","353","338","338","342","342"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","","A++","A++","","","","","","","","","","","","","","","","","","","","","","","","","A++","A++","A","A","A","A","A+","A+"]
["","Capacity","Pdesign","kW","","","","","","","","","3.2","3.2","","","","","","","","","","","","","","","","","","","","","","","","","4.2","4.2","4.50","4.50","4.30","4.30","4.80","4.80"]
["","SCOP/A","","","","","","","","","","","4.64","4.64","","","","","","","","","","","","","","","","","","","","","","","","","4.61","4.61","3.90","3.90","3.86","3.86","4.00","4.00"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","","","2.55","2.55","","","","","","","","","","","","","","","","","","","","","","","","","3.2","3.2","3.55","3.55","3.41","3.41","3.73","3.73"]
["","Annual energy consumption","","kWh/a","","","","","","","","","966","966","","","","","","","","","","","","","","","","","","","","","","","","","1275","1275","1,614","1,614","1,560","1,560","1,680","1,680"]