{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FVA71AMVEB / RZASG71M2V1B","FVA125AMVEB / RZASG125M7V1B","FVA140AMVEB / RZASG140M7V1B","FVA100AMVEB / RZASG100M7V1B (Archived)","FVA71AMVEB / FVA71AMVEB / RZASG140M7V1B (Archived)"]
["Cooling capacity","Nom.","","kW","6.80 (1)","12.1 (1)","13.4 (1)"]
["Space cooling","SEER","","","5.83","5.52","5.63"]
["","Annual energy consumption","","kWh/a","408","1,314","1,428"]
["","Capacity","Pdesign","kW","6.80","12.1","13.4"]
["","Energy efficiency class","","","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","6.00","7.80"]
["","SCOP/A","","","4.04","3.64","3.81"]
["","Energy efficiency class","","","A+"]
["","Annual energy consumption","","kWh/a","1,559","2,308","2,866"]
["Heating capacity","Nom.","","kW","7.50 (2)","13.5 (2)","15.5 (2)"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","9.5","13.4"]
["Heating capacity","Nom.","","kW","","","","10.8","15.5"]
["Space cooling","Energy efficiency class","","","","","","A+"]
["","Capacity","Pdesign","kW","","","","9.5","13.4"]
["","SEER","","","","","","5.72","7.71"]
["","Annual energy consumption","","kWh/a","","","","581","1043"]
["Space heating (Average climate)","Energy efficiency class","","","","","","A"]
["","Capacity","Pdesign","kW","","","","6","7.80"]
["","SCOP/A","","","","","","3.83","4.43"]
["","Annual energy consumption","","kWh/a","","","","2193","2467"]