{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M"]
[]
[]
[]
[]
["","","","","","RXM20M2V1B","RXM25M2V1B","RXM35M2V1B","RXM42M2V1B","RXM50M2V1B","RXM50MV1B","RXM60M2V1B","RXM71M2V1B"]
["Dimensions","Unit","","Height","mm","550","550","550","735","735","735","735","734"]
["","","","Width","mm","765","765","765","825","825","825","825","870"]
["","","","Depth","mm","285","285","285","300","300","300","300","320"]
["Weight","Unit","","","kg","32","32","32","47","47","44","44","56"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10","-10","-10 (1)","-10 (1)","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46 (1)","46 (1)","46","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","49","","","48","48"]
["","","","Nom.","dBA","","","","48","48","","","47"]
["","","","Low","dBA","","","","","","44","44"]
["","Heating","","High","dBA","47","47","49","","","49","49"]
["","","","Nom.","dBA","","","","48","49","","","48"]
["","","","Low","dBA","","","","","","45","45"]
["Refrigerant","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.76","0.76","0.76","1.30","1.40","1.4","1.45","1.15"]
["","Charge","","","tCO2Eq","0.5","0.5","0.5","0.88","0.95","0.9","1.0","0.78"]
["","GWP","","","","675","675","675","675","675","675","675","675.0"]
["Piping connections","Piping length","OU - IU","Max.","m","30","30","30","30","30","30","30","30.0"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","20","20","20","20","20","20","20","20.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","","","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Drain plug","","","","","","","1","1","","","1"]
["Notes","","","","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","","(1) - See separate drawing for operation range"]
["Standard Accessories","Drain cap","","","","","","","","","","","3"]