{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":23,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 4MXM-M"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM50M2V1B / 4MXM68M2V1B","FTXM25M2V1B / FTXM42M2V1B / 4MXM68M2V1B","FTXM35M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / 4MXM68M2V1B","FTXM25M2V1B / FTXM35M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM50M2V1B / 4MXM68M2V1B","FTXM25M2V1B / FTXM25M2V1B / FTXM25M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM35M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM25M2V1B / FTXM25M2V1B / FTXM42M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM25M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM42M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM25M2V1B / 4MXM68M2V1B","FTXM25M2V1B / FTXM25M2V1B / FTXM35M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM50M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM42M2V1B / 4MXM68M2V1B","FTXM20M2V1B / FTXM60M2V1B / 4MXM80M2V1B","FTXM42M2V1B / FTXM42M2V1B / 4MXM80M2V1B"]
["Cooling capacity","Nom.","","kW","6.80","6.70","6.80","6.00","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.50","6.80","6.80","6.80","7.40","8.00"]
["Space cooling","Annual energy consumption","","kWh/a","306","294","297","268","314","313","310","300","310","310","313","309","310","294","313","313","310","351","399"]
["","Capacity","Pdesign","kW","6.80","6.70","6.80","6.00","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.50","6.80","6.80","6.80","7.40","8.40"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","4.30","4.80","5.30","5.30","5.30","5.30","5.80","5.30","5.30","5.30","5.30","5.30","5.30","5.30","5.30","5.30","4.27","4.27"]
["","Pdh Heating capacity at -10°","","kW","0","0","0","","","","","","","","","","","","","","","3.67","3.65"]
["","Annual energy consumption","","kWh/a","1,612","1,559","1,680","1,821","1,765","1,748","1,800","1,757","1,789","1,796","1,775","1,807","1,782","1,814","1,782","1,755","1,789","1,474","1,472"]
["Nominal efficiency","Annual energy consumption","","kWh","794","751","723","665","848","852","879","870","879","892","852","883","874","810","856","865","888","803","903"]
["Heating capacity","Nom.","","kW","8.60","8.30","8.60","7.80","8.60","8.60","8.60","8.60","8.60","8.60","8.60","8.60","8.60","8.20","8.60","8.60","8.60","9.30","9.50"]
["Space cooling","SEER","","","7.78","7.99","8.02","7.84","7.59","7.61","7.70","7.95","7.69","7.69","7.60","7.71","7.68","7.76","7.62","7.61","7.67","7.38","7.38"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","SCOP/A","","","3.90","3.86","4.00","4.07","4.20","4.24","4.12","4.62","4.14","4.13","4.18","4.10","4.16","4.09","4.16","4.22","4.14","4.05","4.06"]
["","Energy efficiency class","","","A","A","A+","A+","A+","A+","A+","A++","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Nominal efficiency","EER","","","4.28","4.46","4.70","4.51","4.01","3.99","3.87","4.41","3.87","3.81","3.99","3.85","3.89","4.01","3.97","3.93","3.83","4.61","4.43"]
["","COP","","","3.82","3.95","3.81","4.56","4.40","4.34","4.32","4.84","4.27","4.22","4.37","4.38","4.29","4.49","4.34","4.30","4.26","3.85","3.73"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]